RTP Payload Formatfor H.263+

April 1998 update

draf t- ietf-av t-rtp-h2 63-vid eo -01.txt

J örg Ott, Univ ersität Bremen TZI

jo@ tzi.org

Changes since -00

¯ Tak e out feedback b ackchannel

˘ draft-ietf-avt-work-in-progress

¯ Changes announced at Washingto n IETF

˘ remove SBIT/EBIT (can use zero bits instead)

˘ unify packet types into one (with extensions)

¯ 16 bits, +8 fo r redund ancy, +1-48 for picture he ader

˘ allow pretty much full H.263+ picture header

˘ elide leading 16 zero bits (P bit)

˘

Changes (2)

¯ Ed itorial cleanups

Summary:

¯ differ ent bits, s ame functionality

¯ mor e efficient representation

We are don e:

¯ two implemen tations

¯ referenced from H.323v2

Ü WG Last Call